**Pre-trip Inspection Requirements:**

*Section 37.22 B.C. Motor Vehicle Act Regulations* states following:

#### “Pre-trip and post-trip inspections

**37.22**   (1)No carrier shall permit a driver to drive, and no driver shall drive, a commercial motor vehicle unless the requirements of this section are met.

(2)The driver or a person specified by the carrier shall be satisfied that the commercial motor vehicle is in a safe operating condition including, but not limited to, the operating condition of the following items:

(a)service brakes, including trailer brake connections and brake adjustments;

(b)parking brake;

(c)steering mechanism;

(d)lighting devices and reflectors;

(e)tires;

(f)horn;

(g)windshield wipers;

(h)rear vision mirrors;

(i)coupling devices;

(j)wheels and rims;

(k)emergency equipment;

(l)load securement devices.

(3)The inspection referred to in subsection (2) shall be performed daily before the first trip of the day.”

Please note that in addition to the above equipment being in working order you must also ensure that the vehicle has a current CVSI sticker, insurance documentation and that the Trip Inspection book is onboard and filled out correctly (including date and bus number on the cover).

**No Go List:**

* Non operational wipers
* Non operational head lamps (minimum 1 lamp in daylight hours and 2 after dark)
* Non operation turn signals
* Non operation brake lights
* Non operation rear running lamps (Minimum 1 in daylight hour and 2 after dark)
* Non operation service brakes or parking brake
* Non operational horn
* Non operational steering mechanism
* Tires with excessive wear (minimum tread 3.2 mm)
* Missing emergency equipment
* Non operational mirrors

Please do not operate any vehicle if any of the above mentioned mechanisms are not working correctly or are missing. Contact Dispatch and request a change off in the yard if discovered during your pre trip or at your current location if failure occurs on the road. You will be the one fined for operating a vehicle that does not meet the requirements.